C rate

Rate at which the capacity of the battery is built up(charged )or given up(discharge )to the load

Ib=C/N

Ib=battery current

N=number hoyrs of continuous discharge

C=Capacity

Supplies Ib current for a give C Ah battery for less than N hours